PAUL
		Help on Using the maps

  The adaptive maps can be uploaded from the ECU so that they can be inspected for
spurious data that could be responsible for poor or erratic running. To do this
choose ECU TOOLS from the menu bar, followed by "upload adaptive map" and "bank1357"
or "bank2468". The adaptive map will then be displayed in numerical and graphical
form. The graph represents one "line" of the map below it. This "line" can be selected by 
"clicking" on to a speed box or throttle position box. E.g. if you click on the 2000 rpm box
all throttle positions at 2000 rpm will be highlighted in blue. This line is shown by the 
blue graph. the red graph shows the previous speed line, the green graph shows the next
speed line. 
  Ideally these lines should stay roughly horizontal and close to 0 % .If values are 
high (>+/-20 %) or erratic, suspect excessive purging , worn/erratic throttle pots, leaks 
in exhaust/intake manifolds, faulty lambda sensors or incorrect fuel pressure (see "real
 time help" for fault screen).
  
   If you wish to save an adaptive map that you have uploaded, "click" on File then on 
Save Map to Disc ."Click" on the filename box and type in your chosen filename followed
by .map  e.g. map1.map 
   You can view a map that has been saved at a later date without the ECU connected. To
do this "click" on File, then on Load Map From Disc, next "click" on the file name you 
wish to view then on the OK box. The map will now be displayed as before.  




